[language]
STRING_Line_Buf_Mark_End_Not_Empty=big error! The segment is not cleared after completion!!!
STRING_FIBER_PWM_NOT_HALF=the frequency cannot be set to 0 and the duty cycle must be equal to 50%
STRING_Ext_Para_OverFlow=motor speed or acceleration out of range
STRING_Card_is_not_connected=Card is not connected
STRING_FUN_Mark_Fail =Mark Fail
STRING_Card_is_Busy_Start_Rask_Fail=Card is Busy,Start Rask Fail
STRING_Layer_number_Over=Layer number Over...
STRING_Data_is_nan=Data is nan...
STRING_PointMark_time_less_than_1=PointMark_time_less_than_1
STRING_Lines_endPoint_less_than_2=Lines endPoint less than 2
STRING_not_Open_OffLine_File=Can't Open OffLine File
STRING_not_Open_Box_File=Can't Open Box File
STRING_UnSuported_Cali_Type=UnSuported Cali Type!!
STRING_Line_Less_Than_1=Line Less Than 1
STRING_OffLineFile_is_too_Big=OffLineFile is too Big
STRING_Fifo_data_error=Fifo data error
STRING_Ext_Axis_number_Over=Ext Axis number Over...
STRING_illige_Call_markFunc_Same_time=illegal calling marking function at the same time!
STRING_mark_not_start=mark not start...
STRING_dotMark_is_illige_for_rotationMark=spot welding does not meet rolling marking requirements
STRING_line_direction_err_for_rotationMark=the line direction does not meet the rolling marking requirements
STRING_mark_error=mark error...
STRING_markTime_not_add=data flow time does not increase in sequence, please contact the supplier!!!
STRING_LineEnegyWaveTooLong=the line energy waveform setting is too long, please confirm whether it is reasonable!
STRING_Card_is_Marking_StopFail=the board is in the running state, failed to abort
STRING_ScanDriveMotor_TimeErr=galvanometer drive motor time is abnormal
STRING_WriteReadFlash_not_same=flash write exception!
STRING_Flush_Fail=parameter update to board is abnormal!
STRING_MarkData_is_not_Locked_to_use=MarkData_is_not_Locked_to_use
STRING_Download_no_Nand= the current board has no offline function
STRING_ERR_UART=serial port received data format is inconsistent
STRING_Laser_is_already_on_when_open=STRING_Laser_is_already_on_when_open
STRING_laser_time_is_Minus=laser_time_is_Minus!
STRING_DllCfg_different_With_Card=DllCfg_different_With_Card!
STRING_Task_Over_Time=Task_Over_Time!
STRING_MarkLaserByIO_illigel_enable_dot_line_both=MarkLaserByIO_illigel_enable_dot_line_both
STRING_MemoryException=out of memory!
STRING_preLaserOff_BigThan_CurLaserOn=preLaserOff_BigThan_CurLaserOn